IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Sanitary_Toilets_DURAVIT_Starck-3-wall-mounted-toilet-252709.ifc"
Time stamp: "2020-02-07T14:16:48"
Author: "Supplier"
Organization: "BIMobject"
Preprocessor: "IFC Engine DLL 2017-09-06"
Originating system: "BIMobject-Lena"
Authorization: "Full Scope"
Application: "BIMobject-Lena" version "0.10" identifier "LTC 110" by Organization "BIMobject" description "BIMobjectï¿½ Corporation"

People and organizations
  Person "Jï¿½nos" "Maros" of Organization "BIMobject" description "BIMobjectï¿½ Corporation"
  Owner history of Person "Jï¿½nos" "Maros" of Organization "BIMobject" description "BIMobjectï¿½ Corporation" | application "BIMobject-Lena" version "0.10" identifier "LTC 110" by Organization "BIMobject" description "BIMobjectï¿½ Corporation" | change ADDED | created 1581085008 (2020-02-07T14:16:48Z) | last modified 1581085008 (2020-02-07T14:16:48Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: STERADIAN
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "BIMobject Library"
  IFCSITE
    IFCBUILDING
      IFCBUILDINGSTOREY | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Starck 3 wall-mounted toilet 252709" | names: "Starck 3 wall-mounted toilet 252709" | property sets: ePset_BIMobjectScript, ePset_BIMobject_BO

Types
  IFCSANITARYTERMINALTYPE "Starck 3 wall-mounted toilet 252709" | 1 occurrence

Property sets
  ePset_BIMobjectScript | properties | on 1 object (1 IFCFLOWTERMINAL)
    Color = "00 White Alpin" (IFCLABEL)
    LOD = "300" (IFCLABEL)
  ePset_BIMobject_BO | properties | on 1 object (1 IFCFLOWTERMINAL)
    BO_classific = "" (IFCTEXT)
    BO_links = "" (IFCTEXT)
    BO_real = "" (IFCTEXT)
    BO_regions = "" (IFCTEXT)
    BimObjectCategory (BO_bocat) = "Toilets" (IFCTEXT)
    BimObjectCategoryCode (BO_bocat_code) = "sanitary-toilets" (IFCTEXT)
    BimObjectMainCategory (BO_bomaincat) = "Sanitary" (IFCTEXT)
    BimObjectMainCategoryCode (BO_bomaincat_code) = "sanitary" (IFCTEXT)
    BrandUrl (BO_brandurl) = "http://www.duravit.com" (IFCTEXT)
    COBIeTypeCategory (BO_cobie_type_cat) = "" (IFCTEXT)
    Depth (BO_depth) = 540. (IFCREAL)
    DesignCountry (BO_designcont) = "" (IFCTEXT)
    EditionNumber (BO_edinum) = 1 (IFCINTEGER)
    GtinCode (BO_gtin) = "4021534984808" (IFCTEXT)
    Height (BO_height) = 375. (IFCREAL)
    IfcClassification (BO_ifcclas) = "Sanitary Terminal" (IFCTEXT)
    InstallationInstructions (BO_montins) = "http://pro.duravit.com/p/252709" (IFCTEXT)
    InstructionVideo (BO_youtube) = "http://pro.duravit.com/p/252709" (IFCTEXT)
    ManufacturCountry (BO_mancont) = "" (IFCTEXT)
    ManufacturName (BO_Manufac) = "DURAVIT" (IFCTEXT)
    MasterFormat2014Code (BO_masterformat2014_code) = "01 52 19" (IFCTEXT)
    MasterFormat2014Description (BO_masterformat2014_name) = "Sanitary Facilities" (IFCTEXT)
    MaterialMain (BO_mainmat) = "Ceramics" (IFCTEXT)
    MaterialSecondary (BO_secmat) = "" (IFCTEXT)
    NBSReference (BO_nbs_ref) = "35-65-90" (IFCTEXT)
    NBSReferenceDescription (BO_nbs_desc) = "Toilet Systems" (IFCTEXT)
    OmniClassCode (BO_omniclass_code) = "23-31 19 00" (IFCTEXT)
    OmniClassDescription (BO_omniclass_name) = "Toilets" (IFCTEXT)
    ProductCertification (BO_prodcert) = "http://pro.duravit.com/p/252709" (IFCTEXT)
    ProductDataUrl (BO_prodaturl) = "bimobject.com/duravit/product/starck-3-wall-mounted-toilet-252709" (IFCTEXT)
    ProductFamily (BO_prodfam) = "Starck 3" (IFCTEXT)
    ProductGroup (BO_prodgroup) = "toilet" (IFCTEXT)
    ProductGuid (BO_productguid) = "1705f2fd-75c3-4a98-ba40-5427de26389a" (IFCTEXT)
    ProductName (BO_prodinfo) = "Starck 3 wall-mounted toilet 252709" (IFCTEXT)
    ProductUrl (BO_producturl) = "http://pro.duravit.com/p/252709" (IFCTEXT)
    PublishDate (BO_publisdat) = "" (IFCTEXT)
    QR (BO_boqrurl) = "http://bimobject.com/duravit/product/starck-3-wall-mounted-toilet-252709" (IFCTEXT)
    RegionAfrica (BO_africa) = "All" (IFCTEXT)
    RegionAntarctica (BO_antarctica) = "All" (IFCTEXT)
    RegionAsia (BO_asia) = "All" (IFCTEXT)
    RegionEurope (BO_europe) = "All" (IFCTEXT)
    RegionMiddleEast (BO_middleeast) = "All" (IFCTEXT)
    RegionNorthAmerica (BO_northamerica) = "All" (IFCTEXT)
    RegionOceania (BO_oceania) = "All" (IFCTEXT)
    RegionSouthAmerica (BO_southamerica) = "All" (IFCTEXT)
    SKU (BO_prodsku) = "starck-3-wall-mounted-toilet-252709" (IFCTEXT)
    TechnicalDescription (BO_techcert) = "http://pro.duravit.com/p/252709" (IFCTEXT)
    UniFormat2Code (BO_uniformat2_code) = "D2030" (IFCTEXT)
    UniFormat2Description (BO_uniformat2_name) = "Sanitary Waste" (IFCTEXT)
    Uniclass14Code (BO_uniclass_1_4_code) = "L7216" (IFCTEXT)
    Uniclass14Description (BO_uniclass_1_4_desc) = "Toilets" (IFCTEXT)
    Uniclass2015Code (BO_uniclass2015_code) = "Pr_40_20_93" (IFCTEXT)
    Uniclass2015Description (BO_uniclass2015_desc) = "Urinal and WC fittings" (IFCTEXT)
    Uniclass20Code (BO_uniclass_2_0_code) = "SS-35-65-90" (IFCTEXT)
    Uniclass20Description (BO_uniclass_2_0_desc) = "Toilet Systems" (IFCTEXT)
    UnspscCode (BO_unspsc) = "301815" (IFCTEXT)
    Weight (BO_weight) = 27. (IFCREAL)
    Width (BO_width) = 365. (IFCREAL)